; ** COPYRIGHT (C) 2007-2018 Realtek CORPORATION
;
; Realtek PCIe FE Family Controller
; Realtek PCI GbE Family Controller
; Realtek PCIe GbE Family Controller
; Realtek PCIe 2.5GbE Family Controller
;
; This product is covered by one or more of the following patents:
; US6,570,884, US6,115,776, and US6,327,625.
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
DriverVer   = 06/15/2018,8.065.0615.2018
CatalogFile.NT = rt630x86.cat

[Manufacturer]
%Realtek%=Realtek, NTx86.6.2, NTamd64.6.2

[ControlFlags]
ExcludeFromSelect     = *

[Realtek]
;Empty section, so this INf does not support win2000

[Realtek.NTamd64.6.2]
;Empty section, so this INf does not support win8 x64

[Realtek.NTx86.6.2]
; 8169
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8169&REV_10


; 8168
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&REV_01
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_01

; 8112
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83851043&REV_01


; 8101
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&REV_01
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_01


; 8131
%RTL8136.DeviceDesc%  = RTL8136.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_83A01043&REV_01


; 8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167
%RTL8169.DeviceDesc%  = RTL8169.ndi, PCI\VEN_10EC&DEV_8167&SUBSYS_816710EC


; 8168C
%RTL8168.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&REV_02
%RTL8168.DeviceDesc%  = RTL8168C.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_02

; 8168C_Force_Gigabit
%RTL8168.DeviceDesc%  = RTL8168CForceGigabit.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83AB1043&REV_02

; 8168CP_Force_100_Full
%RTL8136.DeviceDesc%  = RTL8168CForce100Full.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_2100146C&REV_02


; 8102E
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_02
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_02

;;Compal 8103EL Force Enable Clock Request
%RTL8136.DeviceDesc%  = RTL8102ForceEnableClkReq.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_FF001179&REV_02 ;TOSHIBA


; 8168D
%RTL8168.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&REV_03
%RTL8168.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_03

; 8112L
%RTL8168.DeviceDesc%  = RTL8168D.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_83A31043&REV_03


; 8168DP
%RTL8168.DeviceDesc% = RTL8168DP.ndi, PCI\VEN_10EC&DEV_8168&REV_04
%RTL8168.DeviceDesc% = RTL8168DP.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_04


; 8168E
%RTL8168.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&REV_06
%RTL8168.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_06
%RTL8168.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8161&REV_06 ;Add-on card
%RTL8168.DeviceDesc%  = RTL8168E.ndi, PCI\VEN_10EC&DEV_8161&SUBSYS_816810EC&REV_06 ;Add-on card


; 8168ES
%RTL8168.DeviceDesc%  = RTL8168ES.ndi, PCI\VEN_10EC&DEV_8168&REV_08
%RTL8168.DeviceDesc%  = RTL8168ES.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_08


; 8104
%RTL8136.DeviceDesc%  = RTL8104.ndi, PCI\VEN_10EC&DEV_8137&REV_03
%RTL8136.DeviceDesc%  = RTL8104.ndi, PCI\VEN_10EC&DEV_8137&SUBSYS_813710EC&REV_03


; 8401
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_04
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_04


; 8105E
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_05
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_05


; 8402
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_06
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_06


; 8106E
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&REV_07
%RTL8136.DeviceDesc%  = RTL8105.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_07


; 8106EUS
%RTL8136.DeviceDesc%  = RTL8106EUS.ndi, PCI\VEN_10EC&DEV_8136&REV_08
%RTL8136.DeviceDesc%  = RTL8106EUS.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_08


; 8103EVL
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&REV_09
%RTL8136.DeviceDesc%  = RTL8102.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_09

; 8107E
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&REV_0A
%RTL8136.DeviceDesc%  = RTL8107E.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0A


; 8168F
%RTL8168.DeviceDesc%  = RTL8168F.ndi, PCI\VEN_10EC&DEV_8168&REV_07
%RTL8168.DeviceDesc%  = RTL8168F.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_07


; 8168FB
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_09
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_09

; 8168FR
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_0B
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0B


; 8168G
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8168&REV_0C
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0C
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8161&REV_0C ;Add-on card
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8161&SUBSYS_816810EC&REV_0C ;Add-on card


; 8168GA
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8168&REV_11
%RTL8168.DeviceDesc%  = RTL8168G.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_11


; 8168GU
%RTL8168.DeviceDesc%  = RTL8168GU.ndi, PCI\VEN_10EC&DEV_8168&REV_10
%RTL8168.DeviceDesc%  = RTL8168GU.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_10


; 8168GUA
;%RTL8168.DeviceDesc%  = RTL8168GU.ndi, PCI\VEN_10EC&DEV_8168&REV_13
;%RTL8168.DeviceDesc%  = RTL8168GU.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_13


; 8168H
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&REV_15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_15
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8161&REV_15 ;Add-on card
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8161&SUBSYS_816810EC&REV_15 ;Add-on card

; 8118AS
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_16
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_16

; 8118AS
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&REV_17
%RTL8118.DeviceDesc%  = RTL8118AS.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_17


; 8119
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_18
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_18

; 8119i
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_19
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_19


; 8411
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_0A
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0A


; 8411AAR
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&REV_0F
%RTL8168.DeviceDesc%  = RTL8168FB.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0F


; 8411B
%RTL8168.DeviceDesc%  = RTL8411B.ndi, PCI\VEN_10EC&DEV_8168&REV_12
%RTL8168.DeviceDesc%  = RTL8411B.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_12


; 8411BA
%RTL8168.DeviceDesc%  = RTL8411B.ndi, PCI\VEN_10EC&DEV_8168&REV_14
%RTL8168.DeviceDesc%  = RTL8411B.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_14


; 8168EP
%RTL8168.DeviceDesc%  = RTL8168EP.ndi, PCI\VEN_10EC&DEV_8168&REV_0E
%RTL8168.DeviceDesc%  = RTL8168EP.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0E


; 8168FP
%RTL8168.DeviceDesc%  = RTL8168FP.ndi, PCI\VEN_10EC&DEV_8168&REV_1A
%RTL8168.DeviceDesc%  = RTL8168FP.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1A


; 8168K
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&REV_1B
%RTL8168.DeviceDesc%  = RTL8168H.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1B

; 8125
;%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_00
;%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_00

; 8125AG
;%RTL8125AG.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_01
;%RTL8125AG.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_01

; 8125AP
;%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&REV_02
;%RTL8125.DeviceDesc%  = RTL8125.ndi, PCI\VEN_10EC&DEV_8125&SUBSYS_812510EC&REV_02


; 8168F's successor
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_0D
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_0D
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_13
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_13
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1C
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1C
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1D
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1D
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1E
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1E
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_1F
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_1F
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_20
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_20
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_21
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_21
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_22
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_22
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_23
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_23
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_24
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_24
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_25
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_25
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_26
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_26
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_27
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_27
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&REV_28
%RTL8168.DeviceDesc%  = RTL8168Series.ndi, PCI\VEN_10EC&DEV_8168&SUBSYS_816810EC&REV_28



; 8105E's successor
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0B
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0B
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0C
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0C
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0D
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0D
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0E
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0E
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_0F
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_0F
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_10
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_10
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_11
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_11
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_12
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_12
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_13
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_13
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_14
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_14
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_15
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_15
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_16
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_16
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_17
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_17
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_18
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_18
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_19
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_19
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1A
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1A
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1B
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1B
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1C
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1C
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1D
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1D
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1E
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1E
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&REV_1F
%RTL8136.DeviceDesc%  = RTL8136Series.ndi, PCI\VEN_10EC&DEV_8136&SUBSYS_813610EC&REV_1F


; Realtek
;
; Windows NT specific entry

[R8169C7k.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, JumboNolimit.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe4k.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168Series.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = rtk.reg, Common.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8136.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8136Series.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = rtk.reg, Common.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8136HP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = AutoCrossoverDet.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8136HPS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5woldefaultdisable.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Common.reg, EnablePBA.reg
AddReg          = AutoCrossoverDet.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168C.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg, Rss2Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168CS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg, Rss2Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168CNotSpdDown.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg, Rss2Q.reg
AddReg          = WolS5LinkSpeedNotSpdDown.reg, GreenEthDisabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168CForceGigabit.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed1g.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg, Rss2Q.reg
AddReg          = WolS5LinkSpeedForce1g.reg, GreenEthDisabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168CForce100Full.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = SpeedForce100Full.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe9k.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2.reg, wolptnmagic.reg, rtk.reg, Rss2Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthDisabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8102.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Rss2Q.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8102S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Rss2Q.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8102S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Rss2Q.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8102ForceEnableClkReq.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, ForceEnableClkReq.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, WolShutdownLinkSpeed.reg, Rss2Q.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168D.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168DS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168DS5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168DP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168E.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168ES5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168ES5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168EEEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168EEEEEnS5WOLHideDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168EEEEDnFCDnWMDnWPDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrlDisable.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagicDisable.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEDisable.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168ES.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168F.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FS5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FS5WOLHideDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FS5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FEEEDnS5WOLHideDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEDisable.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FEEEDnFCDn.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrlDisable.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagicDisable.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEDisable.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FB.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, HDSplit.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FBWakeOnLinkUp.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, HDSplit.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
AddReg          = WakeOnLinkUp.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168G.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168GU.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168H.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
AddReg          = GigaLite.reg, GPPSWEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8118AS.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEDisable.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
AddReg          = GigaLite.reg, GPPSWEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8125.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed2.5G.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf8125.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
AddReg          = GigaLite.reg, GPPSWEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8411B.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168EP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8168FP.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Jumboframe9k.reg, OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, GreenEthEnabled.reg, AdvancedEEEDisable.reg
AddReg          = GPPSWEnabled.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8104.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, EnablePBA.reg
AddReg          = WolShutdownLinkSpeed.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8105.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8105S5WOLDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5woldefaultdisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8105S5WOLHideEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhideenable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8105S5WOLHideDisable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg, dels5wol.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wolhidedisable.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8105EEEEnable.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEEEnable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8106EUS.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, AdvancedEEEDisable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3

[RTL8107E.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, s5wol.reg, PDPllEnabled.reg, Common.reg, DisablePBA.reg
AddReg          = OffloadIpv6Lsov2_8102.reg, wolptnmagic.reg, rtk.reg, Rss4Q.reg
AddReg          = WolShutdownLinkSpeed.reg, ArpNsProtOffload.reg, EEE.reg, AdvancedEEEDisable.reg
CopyFiles       = RTL8168.CopyFiles
*IfType         = 6     ; IF_TYPE_ETHERNET_CSMACD
*MediaType      = 0     ; NdisMedium802_3
*PhysicalMediaType = 14     ; NdisPhysicalMedium802_3


[RTL8168.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168Series.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut

[RTL8136.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136Series.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut

[RTL8136HP.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8136HPS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168C.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CNotSpdDown.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CForceGigabit.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168CForce100Full.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8102ForceEnableClkReq.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168D.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DS5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168DP.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168E.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EEEEDnFCDnWMDnWPDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168ES.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168F.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLHideDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FS5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FEEEDnS5WOLHideDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FEEEDnFCDn.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FB.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FBWakeOnLinkUp.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168G.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168GU.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168H.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8118AS.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8125.ndi.NT.HW]
AddReg = RTL8125.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8411B.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168EP.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8168FP.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8104.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLHideEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105S5WOLHideDisable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8105EEEEnable.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8106EUS.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW

[RTL8107E.ndi.NT.HW]
AddReg = RTL8168D.MSI.AddReg
Include = machine.inf
Needs = PciASPMOptOut.HW


[RTL8168_8136.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[RTL8168D.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1

[RTL8125.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 4


[R8169C7k.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8169.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168Series.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8136.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8136Series.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8136HP.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8136HPS5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168C.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168CS5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168CNotSpdDown.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168CForceGigabit.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168CForce100Full.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8102.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8102S5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8102S5WOLHideEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8102ForceEnableClkReq.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168D.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168DS5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168DS5WOLHideEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168DP.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168E.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168ES5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168ES5WOLHideEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168EEEEEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168EEEEEnS5WOLHideDn.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168EEEEDnFCDnWMDnWPDn.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168ES.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168F.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FS5WOLHideEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FS5WOLHideDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FS5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FEEEDnS5WOLHideDn.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FEEEDnFCDn.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FB.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FBWakeOnLinkUp.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168G.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168GU.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168H.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8118AS.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8125.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8411B.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168EP.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8168FP.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8104.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8105.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8105S5WOLDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8105S5WOLHideEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8105S5WOLHideDisable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8105EEEEnable.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8106EUS.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog

[RTL8107E.ndi.NT.Services]
AddService = RTL8168, 2, rtl8168.Service, common.EventLog


;-----------------------------------------------------------------------------
; common base for 10/100/1000 Mb Adapters
;
[Common.reg]
HKR,,DeviceRemovable,0,"0"

HKR,,HwParaMask,0x00010001,0

HKR,,HwOptimize,0x00010001,0

HKR,,HwOption,0x00010001,0

HKR,,HwWolCrcVal,0x00010001,0

HKR,,LogDisconnectEvent,0,"0"

HKR,,EnableEDT,0,"1"

HKR,,RIACP,0,"0"

HKR,,S5NicKeepOverrideMacAddr,0,"0"

HKR,,S5NicKeepOverrideMacAddrV2,0,"1"

HKR,,PPSW,0,"1"

HKR,,GPPSW,0,"0"

HKR,,S0MgcPkt,0,"0"

HKR,,HwFPSM,0x00010001,0

HKR,,SwIML,0x00010001,0

HKR,,ENPWMode,0,"0"

HKR,,Diskless,0,"0"

HKR,,DisklessOption,0,"0"

HKR,,TxOptimizeThreshold,0x00010001,0

HKR,,RxOptimizeThreshold,0x00010001,0

HKR,,CFHTime,0x00010001,0

HKR,,LDWTime,0x00010001,0

HKR,,RMPT,0x00010001,0

HKR,,CRSPDThreshold,0x00010001,0

HKR,,ComboPerfAdjust,0,"0"

HKR,,CHNLWTime,0x00010001,0

HKR,,CHNLWCnt,0x00010001,0

HKR,,L1L0sLT,0x00010001,0

HKR,,MRRSize,0x00010001,0

HKR,,TDBSize,0x00010001,0xFFFFFFFF

HKR,,RDBSize,0x00010001,0xFFFFFFFF

HKR,,HwOptionV2,0x00010001,0

HKR,,HwOptionV3,0x00010001,0

HKR,,HwBpMask,0x00010001,0

HKR,,MonitorModeEnabled,0,"0"

HKR,,UCEM,0x00010001,0

[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

HKR,Ndi\params\AutoDisableGigabit,       ParamDesc,  0, %AutoDisableGigabit%
HKR,Ndi\params\AutoDisableGigabit,       default,    0, "0"
HKR,Ndi\params\AutoDisableGigabit,       optional,   0, "1"
HKR,Ndi\params\AutoDisableGigabit,       type,       0, "enum"
HKR,Ndi\params\AutoDisableGigabit\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoDisableGigabit\enum,  "1",        0, %BatteryRe-Link%
HKR,Ndi\params\AutoDisableGigabit\enum,  "2",        0, %AcBatteryRe-Link%
HKR,,AutoDisableGigabit,0,"0"

[Speed1g.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "6"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"6"

HKR,,ForceMode,0,"0"

[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[SpeedForce100Full.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"4"

HKR,,ForceMode,0,"1"

[Speed2.5G.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2500",     0, %2.5Gb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,,ForceMode,0,"0"

[about.reg]
HKR,,EnumPropPages32,,"rtnicprop32.dll,RTNicPropPageProvider"

[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,     ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,     type,       0, "edit"
HKR,Ndi\params\NetworkAddress,     default,    0, ""
HKR,Ndi\params\NetworkAddress,     LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,     UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,     Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,       ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,       default,    0, "3"
HKR,Ndi\params\*FlowControl,       type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"3"

[flowctrlDisable.reg]
HKR,Ndi\params\*FlowControl,       ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,       default,    0, "0"
HKR,Ndi\params\*FlowControl,       type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "3",        0, %RxTxEnabled%
HKR,,*FlowControl,0,"0"

[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,    ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,    default,    0, "0"
HKR,Ndi\params\*PriorityVLANTag,    type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,   "0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "1",        0, %PriorityEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "2",        0, %VLANEnabled%
HKR,Ndi\params\*PriorityVLANTag\enum,   "3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,    ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,    default,    0, "1"
HKR,Ndi\params\*InterruptModeration,    type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,   "1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[TxRxBuf8125.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "512"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "64"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "4096"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"512"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe4k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,,*JumboPacket,0,"1514"

[Jumboframe9k.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "8192",     0, %8KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "9216",     0, %9KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCbJumboFrame,0,"0"

[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,  ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,       optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[s5woldefaultdisable.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "0"
HKR,Ndi\params\S5WakeOnLan,       optional,   0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"0"

[s5wolhideenable.reg]
HKR,,S5WakeOnLan,0,"1"

[s5wolhidedisable.reg]
HKR,,S5WakeOnLan,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,  ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,  default,    0, "0"
HKR,Ndi\params\*LsoV2IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"0"

HKR,Ndi\params\*LsoV2IPv6,  ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

HKR,Ndi\params\*RSS,    ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,    default,    0, "1"
HKR,Ndi\params\*RSS,    type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"0"

HKR,Ndi\params\*LsoV1IPv4,  ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",       0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",       0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadIpv6Lsov2_8102.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*RSS,    ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,    default,    0, "1"
HKR,Ndi\params\*RSS,    type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"0"

HKR,Ndi\params\*LsoV2IPv4,  ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv4,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"1"

HKR,Ndi\params\*LsoV2IPv6,  ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,  default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,  type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

[AutoCrossoverDet.reg]
HKR,Ndi\params\AutoCrossoverDet,    ParamDesc,  0, %AutoCrossoverDet%
HKR,Ndi\params\AutoCrossoverDet,    default,    0, "0"
HKR,Ndi\params\AutoCrossoverDet,    optional,   0, "1"
HKR,Ndi\params\AutoCrossoverDet,    type,       0, "enum"
HKR,Ndi\params\AutoCrossoverDet\enum,   "0",        0, %Disabled%
HKR,Ndi\params\AutoCrossoverDet\enum,   "1",        0, %Enabled%
HKR,,AutoCrossoverDet,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       optional,   0, "1"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[SSDisable.reg]
HKR,Ndi\params\*SelectiveSuspend,         ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,         default,    0, "0"
HKR,Ndi\params\*SelectiveSuspend,         type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,    "0",        0, %Disabled%
HKR,Ndi\params\*SelectiveSuspend\enum,    "1",        0, %Enabled%
HKR,,*SelectiveSuspend,0,"0"

HKR,Ndi\params\*SSIdleTimeout,      ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,      type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,      default,    0, "50"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"
HKR,Ndi\Params\*SSIdleTimeout,      Base,       0, "10"
HKR,,*SSIdleTimeout,0,"50"

[SSHideDisable.reg]
HKR,,*SelectiveSuspend,0,"0"

HKR,,*SSIdleTimeout,0,"50"

[WolShutdownLinkSpeed.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "0"
HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"0"

[WolS5LinkSpeedNotSpdDown.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "0",    0, %10MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "1",    0, %100MbFirst%
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[WolS5LinkSpeedForce1g.reg]
HKR,Ndi\params\WolShutdownLinkSpeed,    ParamDesc,  0, %WolShutdownLinkSpeed%
HKR,Ndi\params\WolShutdownLinkSpeed,    default,    0, "2"
HKR,Ndi\params\WolShutdownLinkSpeed,    optional,   0, "1"
HKR,Ndi\params\WolShutdownLinkSpeed,    type,       0, "enum"
HKR,Ndi\params\WolShutdownLinkSpeed\enum,   "2",    0, %NotSpeedDown%
HKR,,WolShutdownLinkSpeed,0,"2"

[wolptnmagic.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,  default,    0, "1"
HKR,Ndi\params\*WakeOnPattern,  type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"1"

HKR,Ndi\params\*WakeOnMagicPacket,  ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,  default,    0, "1"
HKR,Ndi\params\*WakeOnMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"1"

[wolptnmagicDisable.reg]
HKR,Ndi\params\*WakeOnPattern,  ParamDesc,  0, %WakeOnPtn%
HKR,Ndi\params\*WakeOnPattern,  default,    0, "0"
HKR,Ndi\params\*WakeOnPattern,  type,       0, "enum"
HKR,Ndi\params\*WakeOnPattern\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnPattern\enum,   "1",        0, %Enabled%
HKR,,*WakeOnPattern,0,"0"

HKR,Ndi\params\*WakeOnMagicPacket,  ParamDesc,  0, %WakeOnMagPkt%
HKR,Ndi\params\*WakeOnMagicPacket,  default,    0, "0"
HKR,Ndi\params\*WakeOnMagicPacket,  type,       0, "enum"
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*WakeOnMagicPacket\enum,   "1",        0, %Enabled%
HKR,,*WakeOnMagicPacket,0,"0"

[GreenEthEnabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "1"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"0"

[GreenEthDisabled.reg]
HKR, Ndi\params\EnableGreenEthernet,        ParamDesc,  0, %GreenEthernet%
HKR, Ndi\params\EnableGreenEthernet,        optional,   0, "1"
HKR, Ndi\params\EnableGreenEthernet,        type,       0, "enum"
HKR, Ndi\params\EnableGreenEthernet,        default,    0, "0"
HKR, Ndi\params\EnableGreenEthernet\enum,   "0",        0, %Disabled%
HKR, Ndi\params\EnableGreenEthernet\enum,   "1",        0, %Enabled%
HKR,,EnableGreenEthernet,0,"0"

[ArpNsProtOffload.reg]
HKR,Ndi\params\*PMARPOffload,       ParamDesc,  0, %ArpOffload%
HKR,Ndi\params\*PMARPOffload,       default,    0, "1"
HKR,Ndi\params\*PMARPOffload,       type,       0, "enum"
HKR,Ndi\params\*PMARPOffload\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*PMARPOffload\enum,  "1",        0, %Enabled%
HKR,,*PMARPOffload,0,"1"

HKR,Ndi\params\*PMNSOffload,        ParamDesc,  0, %NsOffload%
HKR,Ndi\params\*PMNSOffload,        default,    0, "1"
HKR,Ndi\params\*PMNSOffload,        type,       0, "enum"
HKR,Ndi\params\*PMNSOffload\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*PMNSOffload\enum,   "1",        0, %Enabled%
HKR,,*PMNSOffload,0,"1"

[EEE.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        optional,   0, "1"
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "1"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"0"

[EEEEnable.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        optional,   0, "1"
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "1"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"0"

[EEEDisable.reg]
HKR, Ndi\params\*EEE,        ParamDesc,  0, %EEE%
HKR, Ndi\params\*EEE,        optional,   0, "1"
HKR, Ndi\params\*EEE,        type,       0, "enum"
HKR, Ndi\params\*EEE,        default,    0, "0"
HKR, Ndi\params\*EEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\*EEE\enum,   "1",        0, %Enabled%
HKR,,*EEE,0,"0"

[AdvancedEEEEnable.reg]
HKR, Ndi\params\AdvancedEEE,        ParamDesc,  0, %AdvancedEEE%
HKR, Ndi\params\AdvancedEEE,        optional,   0, "1"
HKR, Ndi\params\AdvancedEEE,        type,       0, "enum"
HKR, Ndi\params\AdvancedEEE,        default,    0, "1"
HKR, Ndi\params\AdvancedEEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\AdvancedEEE\enum,   "1",        0, %Enabled%
HKR,,AdvancedEEE,0,"1"

[AdvancedEEEDisable.reg]
HKR, Ndi\params\AdvancedEEE,        ParamDesc,  0, %AdvancedEEE%
HKR, Ndi\params\AdvancedEEE,        optional,   0, "1"
HKR, Ndi\params\AdvancedEEE,        type,       0, "enum"
HKR, Ndi\params\AdvancedEEE,        default,    0, "0"
HKR, Ndi\params\AdvancedEEE\enum,   "0",        0, %Disabled%
HKR, Ndi\params\AdvancedEEE\enum,   "1",        0, %Enabled%
HKR,,AdvancedEEE,0,"0"

[GigaLite.reg]
HKR, Ndi\params\GigaLite,        ParamDesc,  0, %GigaLite%
HKR, Ndi\params\GigaLite,        optional,   0, "1"
HKR, Ndi\params\GigaLite,        type,       0, "enum"
HKR, Ndi\params\GigaLite,        default,    0, "1"
HKR, Ndi\params\GigaLite\enum,   "0",        0, %Disabled%
HKR, Ndi\params\GigaLite\enum,   "1",        0, %Enabled%
HKR,,GigaLite,0,"1"

[HDSplit.reg]
HKR,Ndi\params\*HeaderDataSplit,    ParamDesc,  0, %HDSplit%
HKR,Ndi\params\*HeaderDataSplit,    default,    0, "0"
HKR,Ndi\params\*HeaderDataSplit,    type,       0, "enum"
HKR,Ndi\params\*HeaderDataSplit\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*HeaderDataSplit\enum,   "1",        0, %Enabled%
HKR,,*HeaderDataSplit,0,"0"

[WakeOnLinkUp.reg]
HKR,Ndi\params\WakeOnLinkUp,       ParamDesc,  0, %WakeOnLinkUp%
HKR,Ndi\params\WakeOnLinkUp,       default,    0, "1"
HKR,Ndi\params\WakeOnLinkUp,       optional,   0, "1"
HKR,Ndi\params\WakeOnLinkUp,       type,       0, "enum"
HKR,Ndi\params\WakeOnLinkUp\enum,  "0",        0, %Disabled%
HKR,Ndi\params\WakeOnLinkUp\enum,  "1",        0, %Enabled%
HKR,,WakeOnLinkUp,0,"1"

[WakeOnLinkChgEnable.reg]
HKR, Ndi\params\WakeOnLinkChg,        ParamDesc,  0, %WakeOnLinkChg%
HKR, Ndi\params\WakeOnLinkChg,        optional,   0, "1"
HKR, Ndi\params\WakeOnLinkChg,        type,       0, "enum"
HKR, Ndi\params\WakeOnLinkChg,        default,    0, "1"
HKR, Ndi\params\WakeOnLinkChg\enum,   "0",        0, %Disabled%
HKR, Ndi\params\WakeOnLinkChg\enum,   "1",        0, %Enabled%
HKR,,WakeOnLinkChg,0,"1"

[Rss2Q.reg]
HKR, Ndi\Params\*NumRssQueues,         ParamDesc, 0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,         default,   0, "1"
HKR, Ndi\Params\*NumRssQueues,         type,      0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,    "1",       0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "2",       0, %2Queue%
HKR,,*NumRssQueues,0,"2"

[Rss4Q.reg]
HKR, Ndi\Params\*NumRssQueues,         ParamDesc, 0, %NumRssQueues%
HKR, Ndi\Params\*NumRssQueues,         default,   0, "1"
HKR, Ndi\Params\*NumRssQueues,         type,      0, "enum"
HKR, Ndi\Params\*NumRssQueues\Enum,    "1",       0, %1Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "2",       0, %2Queue%
HKR, Ndi\Params\*NumRssQueues\Enum,    "4",       0, %4Queue%
HKR,,*NumRssQueues,0,"4"

;HKR,,PnPCapabilities,0x10001,0x0000

[PDPllDisabled.reg]
HKR,,PowerDownPll,0,"0"

[PDPllEnabled.reg]
HKR,,PowerDownPll,0,"1"

[DisablePBA.reg]
HKR,,DisablePBA,0,"1"

[EnablePBA.reg]
HKR,,DisablePBA,0,"0"

[ForceEnableClkReq.reg]
HKR,,ForceEnableClkReq,0,"1"

[GPPSWEnabled.reg]
HKR,,GPPSW,0,"1"


[del.reg]
HKR,Ndi\params

HKR,,JumboFrame
HKR,,S3S4WolPowerSaving
HKR,,PowerDownPll
HKR,,*FlowControl
HKR,,*LsoV1IPv4

[dels5wol.reg]
HKR,,S5WakeOnLan


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "RTL8168"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rtl8168.Service]
DisplayName     = %rtl8168.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rt630x86.sys
LoadOrderGroup  = NDIS


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\Rt630x86.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[RTL8168.CopyFiles]
Rt630x86.sys,,,2

[RTLDLL.CopyFiles]
RtNicProp32.dll,,,0x00006000 ; COPYFLG_NOPRUNE | COPYFLG_IN_USE_RENAME

[SourceDisksNames]
1 = %DiskDescription%


[SourceDisksFiles]
Rt630x86.sys = 1,, ; on distribution disk 1
RtNicProp32.dll = 1,, ; on distribution disk 1


[DestinationDirs]
RTL8168.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Realtek                  = "Realtek"
AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
2.5Gb-Full-Duplex        = "2.5 Gbps Full Duplex"
NetworkAddress           = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit"
AutoLinkDownPhyOff       = "Auto Disable PHY"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
8KBMTU                   = "8KB MTU"
9KBMTU                   = "9KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe"
RSS                      = "Receive Side Scaling"
AutoCrossoverDet         = "Auto Crossover Detection"
PriorityEnabled          = "Priority Enabled"
VLANEnabled              = "VLAN Enabled"
10MbFirst                = "10 Mbps First"
100MbFirst               = "100 Mbps First"
WolShutdownLinkSpeed     = "WOL & Shutdown Link Speed"
NotSpeedDown             = "Not Speed Down"
WolCap                   = "Wake-On-Lan Capabilities"
None                     = "None"
PatternMatch             = "Pattern Match"
MagicPacket              = "Magic Packet"
PatternAndMagic          = "Pattern Match & Magic Packet"
GreenEthernet            = "Green Ethernet"
WakeOnPtn                = "Wake on pattern match"
WakeOnMagPkt             = "Wake on Magic Packet"
ARPOffload               = "ARP Offload"
NsOffload                = "NS Offload"
EEE                      = "Energy-Efficient Ethernet"
HDSplit                  = "Header Data Split"
WakeOnLinkUp             = "Wake On Link Up"
NumRssQueues             = "Maximum Number of RSS Queues"
1Queue                   = "1 Queue"
2Queue                   = "2 Queues"
4Queue                   = "4 Queues"
IPSecv2                  = "IPsec Offload"
AH                       = "Auth Header Enabled"
ESP                      = "ESP Enabled"
AHESP                    = "Auth Header & ESP Enabled"
S5ARPOffload             = "Shutdown ARP Offload"
AdvancedEEE              = "Advanced EEE"
GigaLite                 = "Gigabit Lite"
SelectiveSuspend         = "Selective Suspend"
AIPSSelectiveSuspend     = "Advance Idle Power Saving"
SSIdleTimeout            = "Selective Suspend Idle Timeout"
AIPSSSIdleTimeout        = "AIPS Idle Timeout"
WakeOnLinkChg            = "Wake On Link Change"
TeredoOffload            = "Teredo Offload"

RTL8169.DeviceDesc       = "Realtek PCI GbE Family Controller"
RTL8168.DeviceDesc       = "Realtek PCIe GbE Family Controller"
RTL8118.DeviceDesc       = "Realtek Gaming GbE Family Controller"
RTL8136.DeviceDesc       = "Realtek PCIe FE Family Controller"
RTL8125.DeviceDesc       = "Realtek PCIe 2.5GbE Family Controller"
RTL8125AG.DeviceDesc     = "Realtek Gaming 2.5GbE Family Controller"


SMC9452TX.DeviceDesc     = "SMC EZ Card 10/100/1000(SMC9452TX-1)"
DLINKDGE528T.DeviceDesc  = "D-Link DGE-528T Gigabit Ethernet Adapter"
DLINKDGE660TD.DeviceDesc = "D-Link DGE-660TD Gigabit CardBus PC Card"
SITECOM.DeviceDesc       = "Sitecom Gigabit-Ethernet PCI Adapter LN-027"
ZYXELGN680T.DeviceDesc   = "ZyXEL GN680-T Gigabit PCI Adapter"
IODATAETGPCI.DeviceDesc  = "I-O DATA ETG-PCI Gigabit Ethernet Adapter"
IODATAETGCB.DeviceDesc   = "I-O DATA ETG-CB Gigabit Ethernet Adapter"
LGSITV.DeviceDesc        = "LG System Interface(TV)"
TPLINKPCIEGBE.DeviceDesc = "TP-Link Gigabit PCI Express Adapter"

rtl8168.Service.DispName = "Realtek 8168 NT Driver"

DiskDescription      = "Realtek Driver Disk 1"

;;;;; InfVer = 2.000
